This article presents a framework for the automated design optimization of soft sensors using closed-loop 3D printing of a recyclable gelatin hydrogel-based sensing material. The framework facilitates the direct printing of the sensor on the sensing body using RGB-D visual feedback, evaluates the sensor performance, and iteratively improves the sensor design.